TubSure Scotland 18 Mauldslie place Ashgill 07954002957

Service Checklist

Customer Name………………………………………….. Hot Tub model……………………………………………………………

Customer address……………………………………….. Serial Number / year…………………………………………………

…………………………………………………………………… Purchased from…………………………………………………………

…………………………………………………………………… Filter Type…………………………………………………………………

………………………………………………………………….. Filter size…………………………………………………………………

Contact Number ……………………………………….. Current treatment……………………………………………………

Email ……………………………………………………………………………………………………………………………………………….

**Initial Check**

Adequate & Safe Power supply. Check for loose terminals on the PCB

Test water Chlorine/Bromine………………….PH……………. Alkalinity……………….TH………………………….

Comments …………………………………………………………………………………………………………………………………….

**Remove Filter, Open valves and Jets, Add Scale remove and standard flush/Biofilm Flush as required and run System**

Inspect all filters: Clean Filters/ Replace

Remove all access panels and inspect for signs of leaking, rotting, corrosion, rats/rodents

Pumps: No of pumps …………. All pumps operating? Wet ends free from leaks? corrosion

Plumbing: Inspect all pipework for leaks, Unions, Jets, Pump /Heater joints

Have seals been replaced as part of service

Exterior of cabinet: clean……………… Cover: Inspect for tears, Clean……… Replacement advised Yes / No

Comments………………………………………………………………………………………………………………………………………………..

**Drain Hot Tub**

Shell and Interior: Mop out dirty water, apply acrylic cleaner to shell and jets and polish

Pumps: Disconnect pump unions and inspect internals of pump. Replace O rings Yes / No

Heater: Disconnect heater unions and inspect heater element for signs of corrosion

Control Pack: Inspect PCB for signs of Corrosion / Burning

**AMPERAGE DRAW FOR PUMP / HEATER PACK**

Pump1………………………Pump2………………………Pump3…………………….

Heater………………………..Pack…………………………..

**Observation / Recommendation**……………………………………………………………………………………………………………………

Service carried out by …………………………………………..

Customer signature …………………………………………………………………………………..Date…………………………………….